driver + passanger
front left seat + front right seat
MCU 68HC912D60
quartz 4.4..MHz
No need to pull up any pin.
With UPA23 do not write more than one line,
otherwise MCU change value of one byte on
adress 0007h from 42 to C2 and modul is locked
for diagnose.